//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//
.Set READY_VAR = 02
Command ID:	DMR_CC
Send	Command: 84 A9 61 00 02 05 77 0d
Receive	Data:84 A9 61 00 02 05 77 00

Command ID:	DMR_CALL_OPTION
Send	Command: 84 A9 61 00 06 05 79 81 00 00 00 00 
Receive	Data:84 A9 61 00 02 05 79 00
Pause 1000

Command ID:	PROCESS_MODE
Send	Command: 84 A9 61 00 02 00 1A 02
Receive	Data:84 A9 61 00 02 00 1A 00

Command ID:	DEMOD_GAIN
Send	Command: 84 A9 61 00 03 00 1C 00 00
Receive	Command:84 A9 61 00 02 00 1C 00



Command ID:	WORK_MODE_TX
Send	Command: 84 A9 61 00 04 00 18 03 00 00
Receive	Data:84 A9 61 00 02 00 18 00
Command ID:	DMR_CARRIER_LOST
Send	Command: 84 A9 61 00 02 03 19 00
Receive	Data:84 A9 61 00 02 03 19 00
Command ID:	DMR_CARRIER_READY
Send	Command: 84 A9 61 00 02 03 19 {READY_VAR}
Receive	Data:84 A9 61 00 02 03 19 00
//DATA HEAD
Command ID:	DPMR_DATA_FRAME
Send	Command: 84 A9 61 00 0d 05 43 06 0A 82 44 00 00 01 00 00 01 84 00
Receive	Command:84 A9 61 00 01 20 43 

Command ID:	DPMR_DATA_FRAME
Send	Command: 84 A9 61 00 0F 05 43 07 0C 45 00 00 28 00 00 00 00 40 11 8D C3
Receive	Command:84 A9 61 00 01 20 43 

Command ID:	DPMR_DATA_FRAME
Send	Command: 84 A9 61 00 0F 05 43 07 0C 0C 00 00 01 E1 00 00 01 00 00 00 00
Receive	Data:84 A9 61 00 02 30 7F 00
Receive	Data:84 A9 61 00 0F 30 77 0D 43 06 0A 82 44 00 00 01 00 00 01 84 00
Receive	Command:84 A9 61 00 01 20 43 

Command ID:	DPMR_DATA_FRAME
Send	Command: 84 A9 61 00 0F 05 43 07 0C 00 14 7F 66 00 0A A0 00 8C 04 0D 00
Receive	Data:84 A9 61 00 11 30 77 0D 43 07 0C 45 00 00 28 00 00 00 00 40 11 8D C3
Receive	Command:84 A9 61 00 01 20 43 

Command ID:	DPMR_DATA_FRAME
Send	Command: 84 A9 61 00 0F 05 43 07 0c 0A 00 31 00 00 00 00 00 00 00 00 00
Receive	Data:84 A9 61 00 11 30 77 0D 43 07 0C 0C 00 00 01 E1 00 00 01 00 00 00 00
Receive	Command:84 A9 61 00 01 20 43 
Receive	Data:84 A9 61 00 11 30 77 0D 43 07 0C 00 14 7F 66 00 0A A0 00 8C 04 0D 00

Receive	Data:84 A9 61 00 11 30 77 0D 43 07 0C 0A 00 31 00 00 00 00 00 60 57 38 78
Receive	Data:84 A9 61 00 02 20 17 0A
Command ID:	DMR_CARRIER_LOST
Send	Command: 84 A9 61 00 02 03 19 00
Receive	Data:84 A9 61 00 02 03 19 00



