a//Verison=2.2
//Example,Don't Delete flowing text!
//Button NIMI // Generator NIMI 
//Button NIMI 100 // Generator NIMI and Delay 100ms, 100 not is nessary
//Button INT0 // Generator INT0 and Delay 200ms
//Button RESETAMBE3000
//Button RESET3252
//Send 1 command, Receive 2 response with one is not verify.
//Command ID: CARRIER_LOST // necessary!
//Summary  // not essential, 
//Send command: 61 00 02 00 19 00 // necessary!
//Pause=300 // not essential, unit: ms; Pause 300ms after Send command
//Timeout=100 // not essential, unit: ms; if not receive '84 A9 61 ...' in 100ms after send command, Timeout error will happen!
//*Receive Data: 61 00 02 51 19 00 // not essential, receive but not verify
//Receive Data: 61 00 02 51 19 20 // not essential, receive and verify 
//.Set x = AA B0  -- Define var x ; Added in ver2.2
// ... 61 00 02 00 19 {x}   --- use the defined var, The {x} will be replaced with AA B0 
//


Command ID:	CODEC_SELECT at 3700 DPMR bertest need set codec as 31
Send	Command: 84 A9 61 00 02 03 2D 31
Receive	Command:84 A9 61 00 02 03 2D 00
Pause 100
Command ID:	CALL_OPTION
Send	Command: 84 A9 61 00 06 05 47 71 80 00 00 00
Receive	Command:84 A9 61 00 02 05 47 00
Pause 2000


Command ID:	spi3700_freq  428.025Mhz
Send	Command: 84 A9 61 00 03 00 6D 01 b9 00
 Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	spi3700_freq
Send	Command: 84 A9 61 00 03 00 6D 02 c6 00
Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	spi3700_freq
Send	Command: 84 A9 61 00 03 00 6D 03 55 00
Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	spi3700_freq
Send	Command: 84 A9 61 00 03 00 6D 04 b9 00
 Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	spi3700_freq
Send	Command: 84 A9 61 00 03 00 6D 05 c6 00
Receive	Data:84 A9 61 00 02 00 6D 00
Command ID:	spi3700_freq
Send	Command: 84 A9 61 00 03 00 6D 06 55 00
Receive	Data:84 A9 61 00 02 00 6D 00



